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Carpenter safety checklist
Trade-specific safety checks for carpenters - run through before work starts, every time.
	Site address
	[Full site address]

	Date
	[Date]

	Checked by
	[Name]



Checks
	Check
	Yes
	No
	N/A

	Power tool guards in place and working before use
	☐
	☐
	☐

	Dust extraction or mask used when cutting MDF or hardwood
	☐
	☐
	☐

	Manual handling - sheet materials and long timbers carried with assistance
	☐
	☐
	☐

	Working at height - trestles and platforms stable and level
	☐
	☐
	☐

	Electrical safety - 110V tools on site; cables routed away from walkways
	☐
	☐
	☐

	Sharp tools - chisels and blades stored safely, cut away from body
	☐
	☐
	☐

	Fire risk - sawdust cleared regularly; no smoking near timber stores
	☐
	☐
	☐

	Noise - hearing protection when using saws and routers for extended periods
	☐
	☐
	☐

	PPE worn - eye protection, dust mask, safety boots as a minimum
	☐
	☐
	☐

	Site left safe - offcuts cleared, tools secured, area swept
	☐
	☐
	☐



Actions required
[List any issues found and what was done]
Sign-off
	Checked by
	Signature
	Date
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