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Carpenter safety checklist
Trade-specific safety checks for carpenters - run through before work starts, every time.
Site address: ________________________________________________________________________________
Date: ________________________________________________________________________________
Checked by: ________________________________________________________________________________
Checks
[ ] Power tool guards in place and working before use   Yes [ ]   No [ ]   N/A [ ]
[ ] Dust extraction or mask used when cutting MDF or hardwood   Yes [ ]   No [ ]   N/A [ ]
[ ] Manual handling - sheet materials and long timbers carried with assistance   Yes [ ]   No [ ]   N/A [ ]
[ ] Working at height - trestles and platforms stable and level   Yes [ ]   No [ ]   N/A [ ]
[ ] Electrical safety - 110V tools on site; cables routed away from walkways   Yes [ ]   No [ ]   N/A [ ]
[ ] Sharp tools - chisels and blades stored safely, cut away from body   Yes [ ]   No [ ]   N/A [ ]
[ ] Fire risk - sawdust cleared regularly; no smoking near timber stores   Yes [ ]   No [ ]   N/A [ ]
[ ] Noise - hearing protection when using saws and routers for extended periods   Yes [ ]   No [ ]   N/A [ ]
[ ] PPE worn - eye protection, dust mask, safety boots as a minimum   Yes [ ]   No [ ]   N/A [ ]
[ ] Site left safe - offcuts cleared, tools secured, area swept   Yes [ ]   No [ ]   N/A [ ]
Actions required [List any issues found and what was done]
Sign-off
Checked by: ____________________   Signature: ____________________   Date: ____________________
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