
	[image: ]
	[Company name]


How to use this document: delete this paragraph before saving, sharing, or circulating it. Every part shown in blue is yours to replace: type your own details over each blue [field] until no blue remains. Then select all (Ctrl+A) and set the font colour to the same dark colour throughout. What is left is your finished document.
HVAC technician safety checklist
Trade-specific safety checks for hvac technicians - run through before work starts, every time.
Site address: ________________________________________________________________________________
Date: ________________________________________________________________________________
Checked by: ________________________________________________________________________________
Checks
[ ] Refrigerant handling - F-gas certified personnel only; recovery machine available   Yes [ ]   No [ ]   N/A [ ]
[ ] Electrical isolation - unit isolated and proven dead before opening panels   Yes [ ]   No [ ]   N/A [ ]
[ ] Working at height - roof / ladder access risk-assessed; fall protection where needed   Yes [ ]   No [ ]   N/A [ ]
[ ] Manual handling - outdoor units and cylinders moved with aids or assistance   Yes [ ]   No [ ]   N/A [ ]
[ ] Pressure systems - gauges checked; no work on pressurised components without procedure   Yes [ ]   No [ ]   N/A [ ]
[ ] Ventilation - no refrigerant release in confined spaces   Yes [ ]   No [ ]   N/A [ ]
[ ] Hot surfaces - compressor and pipework allowed to cool before handling   Yes [ ]   No [ ]   N/A [ ]
[ ] PPE worn - gloves and eye protection when handling refrigerant or brazing   Yes [ ]   No [ ]   N/A [ ]
[ ] Brazing - hot works permit, fire extinguisher at hand, nitrogen purge used   Yes [ ]   No [ ]   N/A [ ]
[ ] Site left safe - panels refitted, system tested, area clean   Yes [ ]   No [ ]   N/A [ ]
Actions required [List any issues found and what was done]
Sign-off
Checked by: ____________________   Signature: ____________________   Date: ____________________
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