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Painter safety checklist
Trade-specific safety checks for painters - run through before work starts, every time.
Site address: ________________________________________________________________________________
Date: ________________________________________________________________________________
Checked by: ________________________________________________________________________________
Checks
[ ] Ladder safety - ladders footed or tied; no overreaching; 3 points of contact   Yes [ ]   No [ ]   N/A [ ]
[ ] Working at height - towers assembled per instructions; guardrails where required   Yes [ ]   No [ ]   N/A [ ]
[ ] Ventilation - adequate airflow when using solvent-based paints   Yes [ ]   No [ ]   N/A [ ]
[ ] Lead paint awareness - pre-1978 surfaces tested before sanding or stripping   Yes [ ]   No [ ]   N/A [ ]
[ ] Dust - mask worn when sanding; dust sheets contain spread   Yes [ ]   No [ ]   N/A [ ]
[ ] Slips - paint spills cleaned immediately; sheeting secured   Yes [ ]   No [ ]   N/A [ ]
[ ] Manual handling - full paint tins and ladders carried safely   Yes [ ]   No [ ]   N/A [ ]
[ ] Electrical safety - no painting around live fittings without isolation   Yes [ ]   No [ ]   N/A [ ]
[ ] PPE worn - eye protection when stripping, gloves with solvents, dust mask   Yes [ ]   No [ ]   N/A [ ]
[ ] Site left safe - lids on tins, brushes cleaned or stored, area tidy   Yes [ ]   No [ ]   N/A [ ]
Actions required [List any issues found and what was done]
Sign-off
Checked by: ____________________   Signature: ____________________   Date: ____________________
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