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Roofer safety checklist
Trade-specific safety checks for roofers - run through before work starts, every time.
Site address: ________________________________________________________________________________
Date: ________________________________________________________________________________
Checked by: ________________________________________________________________________________
Checks
[ ] Working at height - edge protection or scaffold in place before access   Yes [ ]   No [ ]   N/A [ ]
[ ] Fragile roofs - crawling boards used; no walking on unsupported areas   Yes [ ]   No [ ]   N/A [ ]
[ ] Weather - work stops in high wind, ice, or heavy rain   Yes [ ]   No [ ]   N/A [ ]
[ ] Falling objects - exclusion zone below; toe boards and debris netting   Yes [ ]   No [ ]   N/A [ ]
[ ] Ladders - secured at top, correct angle, inspected before use   Yes [ ]   No [ ]   N/A [ ]
[ ] Manual handling - tile bundles and lead rolls lifted with aids or assistance   Yes [ ]   No [ ]   N/A [ ]
[ ] Overhead lines - minimum clearance checked where present   Yes [ ]   No [ ]   N/A [ ]
[ ] Asbestos - old soffits, flues or cement sheets sampled before disturbance   Yes [ ]   No [ ]   N/A [ ]
[ ] Hot works - permit for torch-on felt; extinguisher at hand   Yes [ ]   No [ ]   N/A [ ]
[ ] PPE worn - harness where required, hard hat, gloves, safety boots   Yes [ ]   No [ ]   N/A [ ]
Actions required [List any issues found and what was done]
Sign-off
Checked by: ____________________   Signature: ____________________   Date: ____________________
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